16 BIT ADDITION

PROGRAM:

LHLD 2500

XCHG

LHLD 2504

MOV A,E

ADD L

MOV L,A

MOV A,D

ADC H

MOV H,A

SHLD 2508

HLT

OUTPUT:

