8 BIT MULTIPLICATION

PROGRAM:

LDA 4051

MOV 4052 B,A

MOV LDA 4052

MOV C,A

MVI A,00H

LOOP: ADD B

DCR C

JNZ LOOP

STA 4053

HLT

OUTPUT:

