8 BIT ADDITION

PROGRAM:

LDA 3052

MOV B,A

LDA 3054

ADD B

STA 3056

HLT

OUTPUT: